--- a/tn7atm.c
+++ b/tn7atm.c
@@ -67,7 +67,7 @@
 #include <linux/atmdev.h>
 #include <linux/delay.h>
 #include <linux/spinlock.h>
-#include <linux/smp_lock.h>
+#include <linux/interrupt.h>
 #include <linux/proc_fs.h>
 #include <linux/string.h>
 #include <linux/ctype.h>
--- a/tn7sar.c
+++ b/tn7sar.c
@@ -48,7 +48,7 @@
 #include <linux/atmdev.h>
 #include <linux/delay.h>
 #include <linux/spinlock.h>
-#include <linux/smp_lock.h>
+#include <linux/interrupt.h>
 #include <linux/proc_fs.h>
 #include <linux/string.h>
 #include <linux/ctype.h>
--- a/tn7dsl.c
+++ b/tn7dsl.c
@@ -100,7 +100,7 @@
 #include <linux/atmdev.h>
 #include <linux/delay.h>
 #include <linux/spinlock.h>
-#include <linux/smp_lock.h>
+#include <linux/interrupt.h>
 #include <linux/proc_fs.h>
 #include <linux/string.h>
 #include <linux/ctype.h>
