#!/bin/sh

. /lib/functions.sh
. /lib/ramips.sh
. /lib/functions/uci-defaults.sh
. /lib/functions/system.sh

ramips_setup_rt3x5x_vlans()
{
	if [ ! -x /sbin/swconfig ]; then
		# legacy default
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		return
	fi
	local wanports=""
	local lanports=""
	for port in 5 4 3 2 1 0; do
		if [ `swconfig dev rt305x port $port get disable` = "1" ]; then
			continue
		fi
		if [ `swconfig dev rt305x port $port get lan` = "0" ]; then
			wanports="$port $wanports"
		else
			lanports="$port $lanports"
		fi
	done
	ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
	ucidef_add_switch "rt305x" "1" "1"
	ucidef_add_switch_vlan "rt305x" "1" "$lanports 6t"
	ucidef_add_switch_vlan "rt305x" "2" "$wanports 6t"
}

ramips_setup_interfaces()
{
	local board="$1"

	ucidef_set_interface_loopback

	case $board in
	3g300m | \
	w150m | \
	all0256n | \
	all5002 | \
	all5003 | \
	broadway | \
	dcs-930| \
	ncs601w | \
	wnce2001)
		ucidef_add_switch "switch0" "1" "0"
		ucidef_set_interface_lan "eth0"
		;;

	3g-6200nl | \
	mlw221)
                ucidef_set_interface_lan "eth0.2"
                ;;

	wl-330n | \
	wmr300)
		ucidef_set_interface_lan "eth0.1"
		;;

	3g-6200n | \
	b2c | \
	nw718 | \
	psr-680w | \
	sl-r7205 | \
	w502u | \
	wr6202)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		;;

	awapn2403)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "0 6t"
		ucidef_add_switch_vlan "switch0" "2" "1 6t"
		;;

	br-6475nd)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "1 2 3 4 9t"
		ucidef_add_switch_vlan "switch0" "2" "0 9t"
		;;

	asl26555)
		ucidef_set_interface_lan "eth0.1"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "1 2 3 4 6t"
		;;

	cy-swr1100)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "0 1 2 3 9t"
		ucidef_add_switch_vlan "switch0" "2" "4 9t"
		;;

	dir-610-a1 | \
	dir-300-b7 | \
	dir-320-b1 | \
	dir-615-h1 | \
	hlk-rm04 | \
	mzk-w300nh2 | \
	mzk-750dhp)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "0 1 2 3 6t"
		ucidef_add_switch_vlan "switch0" "2" "4 6t"
		;;

	awm002-evb | \
	awm003-evb | \
	argus-atp52b | \
	dir-645 | \
	f5d8235-v1 | \
	f5d8235-v2 | \
	hg255d | \
	rt-n14u | \
	wrtnode | \
	ur-326n4g | \
	zbt-wa05)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "1 2 3 4 6t"
		ucidef_add_switch_vlan "switch0" "2" "0 6t"
		;;

	ur-336un)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		;;

	br6524n | \
	v11st-fe)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "1 2 3 4 5t"
		ucidef_add_switch_vlan "switch0" "2" "0 5t"
		;;

	ar725w | \
	rt-n15 | \
	wl-351)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "0 1 2 3 5t"
		ucidef_add_switch_vlan "switch0" "2" "4 5t"
		;;

	rt-n56u)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "0 1 2 3 8t"
		ucidef_add_switch_vlan "switch0" "2" "4 8t"
		;;

	tew-691gr|\
	tew-692gr)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "0t 1 2 3 4"
		ucidef_add_switch_vlan "switch0" "2" "0t 5"
		;;

	wcr-150gn)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "0 6t"
		ucidef_add_switch_vlan "switch0" "2" "6t"
		;;

	wr8305rt)
		ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		ucidef_add_switch "switch0" "1" "1"
		ucidef_add_switch_vlan "switch0" "1" "0 1 2 3 4 6t"
		ucidef_add_switch_vlan "switch0" "2" "4 6t"
		;;

	d105 | \
	na930 | \
	omni-emb-hpm|\
	wli-tx4-ag300n)
		ucidef_set_interface_lan "eth0"
		;;

	*)
		RT3X5X=`cat /proc/cpuinfo | egrep "(RT3.5|RT5350)"`
		if [ -n "${RT3X5X}" ]; then
			ramips_setup_rt3x5x_vlans
		else
			ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
		fi
		;;
	esac
}

ramips_setup_macs()
{
	local board="$1"
	local lan_mac=""
	local wan_mac=""

	case $board in
	br-6475nd)
		lan_mac=$(cat /sys/class/net/eth0/address)
		wan_mac=$(mtd_get_mac_binary devdata 7)
		;;

	w306r-v20)
		lan_mac=$(cat /sys/class/net/eth0/address)
		wan_mac=$(macaddr_add "$lan_mac" 5)
		;;

	tew-691gr)
		lan_mac=$(cat /sys/class/net/eth0/address)
		wan_mac=$(macaddr_add "$lan_mac" 3)
		;;

	tew-692gr)
		lan_mac=$(cat /sys/class/net/eth0/address)
		wan_mac=$(macaddr_add "$lan_mac" 4)
		;;

	m3 |\
	m4 |\
	x5 |\
	x8)
		lan_mac=$(cat /sys/class/net/eth0/address)
		lan_mac=$(macaddr_add "$lan_mac" -2)
		;;

	bc2 |\
	broadway |\
	d105 |\
	dir-620-a1 |\
	esr-9753 |\
	freestation5 |\
	hlk-rm04 | \
	mpr-a1 | \
	mpr-a2 | \
	dir-300-b7 | \
	dir-320-b1 | \
	psr-680w |\
	sl-r7205)
		lan_mac=$(cat /sys/class/net/eth0/address)
		lan_mac=$(macaddr_setbit_la "$lan_mac")
		wan_mac=$(macaddr_add "$lan_mac" 1)
		;;

	cy-swr1100 | \
	dir-645)
		lan_mac=$(mtd_get_mac_ascii nvram lanmac)
		wan_mac=$(mtd_get_mac_ascii nvram wanmac)
		;;

	wcr-150gn)
                wan_mac=$(mtd_get_mac_binary factory 40)
		;;

	rt-n56u)
		lan_mac=$(cat /sys/class/net/eth0/address)
		lan_mac=$(macaddr_setbit_la "$lan_mac")
		wan_mac=$(mtd_get_mac_binary factory 32772)
		;;

	all0239-3g | \
	carambola | \
	freestation5 | \
	w502u | \
	wnce2001)
		wan_mac=$(mtd_get_mac_binary factory 46)
		;;

	*)
		lan_mac=$(cat /sys/class/net/eth0/address)
		wan_mac=$(macaddr_add "$lan_mac" 1)
		;;

	esac

	[ -n "$lan_mac" ] && ucidef_set_interface_macaddr lan $lan_mac
	[ -n "$wan_mac" ] && ucidef_set_interface_macaddr wan $wan_mac
}

[ -e /etc/config/network ] && exit 0

touch /etc/config/network

board=$(ramips_board_name)

ramips_setup_interfaces $board
ramips_setup_macs $board

uci commit network

exit 0
