--- a/arch/powerpc/boot/dts/mpc8548cds.dtsi
+++ b/arch/powerpc/boot/dts/mpc8548cds.dtsi
@@ -293,8 +293,10 @@
 				#address-cells = <0>;
 				#interrupt-cells = <2>;
 				compatible = "chrp,iic";
+/*
 				interrupts = <0 1 0 0>;
 				interrupt-parent = <&mpic>;
+*/
 			};
 
 			rtc@70 {
