From 2d17c793a9cd3f67351d1a15c099ef2464e81f47 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Mon, 20 May 2013 20:30:11 +0200
Subject: [PATCH 13/25] MIPS: ralink: mt7620: add verbose ram info

Make the code print which of SDRAM, DDR1 or DDR2 was detected.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 arch/mips/ralink/mt7620.c |    3 +++
 1 file changed, 3 insertions(+)

--- a/arch/mips/ralink/mt7620.c
+++ b/arch/mips/ralink/mt7620.c
@@ -214,16 +214,19 @@ void prom_soc_init(struct ralink_soc_inf
 
 	switch (dram_type) {
 	case SYSCFG0_DRAM_TYPE_SDRAM:
+		pr_info("Board has SDRAM\n");
 		soc_info->mem_size_min = MT7620_SDRAM_SIZE_MIN;
 		soc_info->mem_size_max = MT7620_SDRAM_SIZE_MAX;
 		break;
 
 	case SYSCFG0_DRAM_TYPE_DDR1:
+		pr_info("Board has DDR1\n");
 		soc_info->mem_size_min = MT7620_DDR1_SIZE_MIN;
 		soc_info->mem_size_max = MT7620_DDR1_SIZE_MAX;
 		break;
 
 	case SYSCFG0_DRAM_TYPE_DDR2:
+		pr_info("Board has DDR2\n");
 		soc_info->mem_size_min = MT7620_DDR2_SIZE_MIN;
 		soc_info->mem_size_max = MT7620_DDR2_SIZE_MAX;
 		break;
