--- a/arch/mips/bcm47xx/leds.c
+++ b/arch/mips/bcm47xx/leds.c
@@ -35,6 +35,15 @@ bcm47xx_leds_asus_rtn12[] __initconst =
 };
 
 static const struct gpio_led
+bcm47xx_leds_asus_rtn15u[] __initconst = {
+	/* TODO: Add "wlan" LED */
+	BCM47XX_GPIO_LED(3, "blue", "wan", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(4, "blue", "lan", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(6, "blue", "power", 1, LEDS_GPIO_DEFSTATE_ON),
+	BCM47XX_GPIO_LED(9, "blue", "usb", 0, LEDS_GPIO_DEFSTATE_OFF),
+};
+
+static const struct gpio_led
 bcm47xx_leds_asus_rtn16[] __initconst = {
 	BCM47XX_GPIO_LED(1, "blue", "power", 1, LEDS_GPIO_DEFSTATE_ON),
 	BCM47XX_GPIO_LED(7, "blue", "wlan", 0, LEDS_GPIO_DEFSTATE_OFF),
@@ -42,8 +51,8 @@ bcm47xx_leds_asus_rtn16[] __initconst =
 
 static const struct gpio_led
 bcm47xx_leds_asus_rtn66u[] __initconst = {
-	BCM47XX_GPIO_LED(12, "unk", "power", 1, LEDS_GPIO_DEFSTATE_ON),
-	BCM47XX_GPIO_LED(15, "unk", "usb", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(12, "blue", "power", 1, LEDS_GPIO_DEFSTATE_ON),
+	BCM47XX_GPIO_LED(15, "blue", "usb", 1, LEDS_GPIO_DEFSTATE_OFF),
 };
 
 static const struct gpio_led
@@ -216,8 +225,8 @@ bcm47xx_leds_linksys_e1000v1[] __initcon
 
 static const struct gpio_led
 bcm47xx_leds_linksys_e1000v21[] __initconst = {
-	BCM47XX_GPIO_LED(5, "unk", "wlan", 0, LEDS_GPIO_DEFSTATE_OFF),
-	BCM47XX_GPIO_LED(6, "unk", "power", 1, LEDS_GPIO_DEFSTATE_ON),
+	BCM47XX_GPIO_LED(5, "blue", "wlan", 0, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(6, "blue", "power", 1, LEDS_GPIO_DEFSTATE_ON),
 	BCM47XX_GPIO_LED(7, "amber", "wps", 0, LEDS_GPIO_DEFSTATE_OFF),
 	BCM47XX_GPIO_LED(8, "blue", "wps", 0, LEDS_GPIO_DEFSTATE_OFF),
 };
@@ -314,6 +323,16 @@ bcm47xx_leds_linksys_wrt54g_type_0101[]
 	BCM47XX_GPIO_LED(7, "green", "dmz", 1, LEDS_GPIO_DEFSTATE_OFF),
 };
 
+/* Verified on: WRT54GL V1.1 */
+static const struct gpio_led
+bcm47xx_leds_linksys_wrt54g_type_0467[] __initconst = {
+	BCM47XX_GPIO_LED(0, "green", "wlan", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(1, "green", "power", 0, LEDS_GPIO_DEFSTATE_ON),
+	BCM47XX_GPIO_LED(2, "white", "wps", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(3, "orange", "wps", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(7, "green", "dmz", 1, LEDS_GPIO_DEFSTATE_OFF),
+};
+
 static const struct gpio_led
 bcm47xx_leds_linksys_wrt610nv1[] __initconst = {
 	BCM47XX_GPIO_LED(0, "unk", "usb",  1, LEDS_GPIO_DEFSTATE_OFF),
@@ -333,11 +352,10 @@ bcm47xx_leds_linksys_wrt610nv2[] __initc
 
 static const struct gpio_led
 bcm47xx_leds_linksys_wrtsl54gs[] __initconst = {
-	BCM47XX_GPIO_LED(0, "unk", "wlan", 1, LEDS_GPIO_DEFSTATE_OFF),
-	BCM47XX_GPIO_LED(1, "unk", "power", 0, LEDS_GPIO_DEFSTATE_ON),
-	BCM47XX_GPIO_LED(2, "white", "wps", 1, LEDS_GPIO_DEFSTATE_OFF),
-	BCM47XX_GPIO_LED(3, "orange", "wps", 1, LEDS_GPIO_DEFSTATE_OFF),
-	BCM47XX_GPIO_LED(7, "unk", "dmz", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(0, "green", "dmz", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(1, "green", "power", 0, LEDS_GPIO_DEFSTATE_ON),
+	BCM47XX_GPIO_LED(5, "white", "wps", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(7, "orange", "wps", 1, LEDS_GPIO_DEFSTATE_OFF),
 };
 
 /* Motorola */
@@ -385,6 +403,15 @@ bcm47xx_leds_netgear_wndr4500v1[] __init
 };
 
 static const struct gpio_led
+bcm47xx_leds_netgear_wnr3500lv1[] __initconst = {
+	BCM47XX_GPIO_LED(0, "blue", "wlan", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(1, "green", "wps", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(2, "green", "wan", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(3, "green", "power", 0, LEDS_GPIO_DEFSTATE_ON),
+	BCM47XX_GPIO_LED(7, "amber", "power", 0, LEDS_GPIO_DEFSTATE_OFF),
+};
+
+static const struct gpio_led
 bcm47xx_leds_netgear_wnr834bv2[] __initconst = {
 	BCM47XX_GPIO_LED(2, "green", "power", 0, LEDS_GPIO_DEFSTATE_ON),
 	BCM47XX_GPIO_LED(3, "amber", "power", 0, LEDS_GPIO_DEFSTATE_OFF),
@@ -425,6 +452,9 @@ void __init bcm47xx_leds_register(void)
 	case BCM47XX_BOARD_ASUS_RTN12:
 		bcm47xx_set_pdata(bcm47xx_leds_asus_rtn12);
 		break;
+	case BCM47XX_BOARD_ASUS_RTN15U:
+		bcm47xx_set_pdata(bcm47xx_leds_asus_rtn15u);
+		break;
 	case BCM47XX_BOARD_ASUS_RTN16:
 		bcm47xx_set_pdata(bcm47xx_leds_asus_rtn16);
 		break;
@@ -553,6 +583,8 @@ void __init bcm47xx_leds_register(void)
 		bcm47xx_set_pdata(bcm47xx_leds_linksys_wrt54g_type_0101);
 		break;
 	case BCM47XX_BOARD_LINKSYS_WRT54G_TYPE_0467:
+		bcm47xx_set_pdata(bcm47xx_leds_linksys_wrt54g_type_0467);
+		break;
 	case BCM47XX_BOARD_LINKSYS_WRT54G_TYPE_0708:
 		bcm47xx_set_pdata(bcm47xx_leds_linksys_wrt54g_generic);
 		break;
@@ -582,6 +614,9 @@ void __init bcm47xx_leds_register(void)
 	case BCM47XX_BOARD_NETGEAR_WNDR4500V1:
 		bcm47xx_set_pdata(bcm47xx_leds_netgear_wndr4500v1);
 		break;
+	case BCM47XX_BOARD_NETGEAR_WNR3500L:
+		bcm47xx_set_pdata(bcm47xx_leds_netgear_wnr3500lv1);
+		break;
 	case BCM47XX_BOARD_NETGEAR_WNR834BV2:
 		bcm47xx_set_pdata(bcm47xx_leds_netgear_wnr834bv2);
 		break;
--- a/arch/mips/bcm47xx/buttons.c
+++ b/arch/mips/bcm47xx/buttons.c
@@ -329,6 +329,12 @@ bcm47xx_buttons_netgear_wndr4500v1[] __i
 };
 
 static const struct gpio_keys_button
+bcm47xx_buttons_netgear_wnr3500lv1[] __initconst = {
+	BCM47XX_GPIO_KEY(4, KEY_RESTART),
+	BCM47XX_GPIO_KEY(6, KEY_WPS_BUTTON),
+};
+
+static const struct gpio_keys_button
 bcm47xx_buttons_netgear_wnr834bv2[] __initconst = {
 	BCM47XX_GPIO_KEY(6, KEY_RESTART),
 };
@@ -538,6 +544,9 @@ int __init bcm47xx_buttons_register(void
 	case BCM47XX_BOARD_NETGEAR_WNDR4500V1:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_netgear_wndr4500v1);
 		break;
+	case BCM47XX_BOARD_NETGEAR_WNR3500L:
+		err = bcm47xx_copy_bdata(bcm47xx_buttons_netgear_wnr3500lv1);
+		break;
 	case BCM47XX_BOARD_NETGEAR_WNR834BV2:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_netgear_wnr834bv2);
 		break;
