/*
 * Copyright (C) 2014 STMicroelectronics R&D Limited
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */
/ {
	clocks {
		/*
		 * Fixed 30MHz oscillator inputs to SoC
		 */
		clk_sysin: clk-sysin {
			#clock-cells = <0>;
			compatible = "fixed-clock";
			clock-frequency = <30000000>;
		};

		/*
		 * ARM Peripheral clock for timers
		 */
		arm_periph_clk: arm-periph-clk {
			#clock-cells = <0>;
			compatible = "fixed-clock";
			clock-frequency = <600000000>;
		};

		/*
		 * Bootloader initialized system infrastructure clock for
		 * serial devices.
		 */
		clk_ext2f_a9: clockgen-c0@13 {
			#clock-cells = <0>;
			compatible = "fixed-clock";
			clock-frequency = <200000000>;
			clock-output-names = "clk-s-icn-reg-0";
		};
	};
};
