/*
 * Copyright (C) 2012 Texas Instruments Incorporated - http://www.ti.com/
 * Copyright (C) 2014 Stefan Roese <sr@denx.de>
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

#include "omap3-ha-common.dtsi"

/ {
	model = "TI OMAP3 HEAD acoustics baseboard with TAO3530 SOM";
	compatible = "headacoustics,omap3-ha", "technexion,omap3-tao3530", "ti,omap34xx", "ti,omap3";
};

&omap3_pmx_core {
	pinctrl-names = "default";
	pinctrl-0 = <
		&hsusbb2_pins
		&powerdown_input_pins
		&fpga_boot0_pins
		&fpga_boot1_pins
		&led_blue_pins
		&led_green_pins
		&led_red_pins
	>;
};
