# short-description: Create a 'pcbios' direct disk image
# long-description: Creates a partitioned legacy BIOS disk image that the user
# can directly dd to boot media.


part /boot --source bootimg --ondisk sda --fstype=msdos --label boot --active --align 1024
part / --source rootfs --ondisk sda --fstype=ext3 --label platform --align 1024

bootloader  --timeout=0  --append="rootwait rootfstype=ext3 video=vesafb vga=0x318 console=tty0"

